{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["一层"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"一层","index":0,"n_rows":170,"n_cols":6,"rows_kept":170,"merged":[[0,0,0,5],[1,0,1,5],[3,1,3,5],[85,0,85,5],[87,0,87,5],[107,0,107,5],[117,0,117,5],[145,0,145,5],[163,0,163,5]],"flags":["formulas_cached_only"]}
["山西煤机装备制造有限责任公司厨房设备设施技术要求"]
["   一层"]
["编号","名称","规格","单位","数量","技术参数"]
[null,"      厨房"]
[1,"调料台","300*1100*800","台",2,"高强度不锈钢板，主体用1.5mm不锈钢板材，脚为直径50mm*壁厚1.2mm不锈钢圆管，可调节重力子弹脚，防割手。"]
[2,"双炒双温灶","2000*1100*800","台",2,"灶面1.5mm厚优质不锈钢板，其它为1.2mm，炉体主架采用3.0mm钢板和38*38方管焊接；灶腿直径50mm钢管；灶腿高度可调；节能静音灶头。带熄火保护。"]
[3,"异形调料台","660*500*800","台",1,"高强度不锈钢板，主体用1.5mm不锈钢板材，脚为直径50mm*壁厚1.2mm不锈钢圆管，可调节重力子弹脚，防割手。"]
[4,"单炒单温灶","1000*1100*800","台",1,"灶面1.5mm厚优质不锈钢板，其它为1.2mm，炉体主架采用3.0mm钢板和38*38方管焊接；灶腿直径50mm钢管；灶腿高度可调；节能静音灶头。带熄火保护。"]
[5,"调料台","400*1100*800","台",1,"高强度不锈钢板，主体用1.5mm不锈钢板材，脚为直径50mm*壁厚1.2mm不锈钢圆管，可调节重力子弹脚，防割手。"]
[6,"大锅灶","1100*1100*800","台",2,"灶面1.5mm厚优质不锈钢，其它为1.2mm，衬板≥3.0mm不锈钢板。主支架≥40mm*40mm*4mm不锈钢角钢焊接，带熄火保护。单头用气量≤3.5m3/h。风机采用铜芯优质电机，电源为220V/50HZ，噪声：≤65dB。\n"]
[7,"调料台","440*1100*800","台",1,"高强度不锈钢板，主体用1.5mm不锈钢板材，脚为直径50mm*壁厚1.2mm不锈钢圆管，可调节重力子弹脚，防割手。"]
[8,"双眼低汤灶","1200*700*600","台",1,"灶面1.5mm厚优质不锈钢板，其它为1.2mm，炉体主架采用3.0mm钢板和38*38方管焊接；灶腿直径50mm钢管；灶腿高度可调；节能静音灶头。带熄火保护。"]
[9,"海鲜蒸柜","910*910","台",1,"面板采用1.5mm厚优质不锈钢板，其它为1.2mm，主架2.0mm钢板和38*38方管焊接，灶膛采用2.0mm不锈钢板。国标无缝燃气气管，防腐、防锈处理；炉火燃烧值不低于48000大卡/小时。配有熄火保护。"]
[10,"三星水池","1800*700*800","台",1,"采用高强度不锈钢板1.35mm，星盆为一次冲压成型，配备不锈钢过滤、防臭下水漏；支撑腿厚度1.2mm,直径为50mm圆钢,可调节高度不锈钢子弹脚。"]
[11,"热水器","80L","台",1,"名牌，功率3KW"]
[12,"双层工作台","2000*1000*800","台",2,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[13,"单通工作柜","2000*1000*800","台",3,"优质不锈钢制造，主体1.5mm不锈钢板材，下滑轮冲压轨道门，中间层板1.2mm，配备可调式不锈钢子弹脚，直径50mm，防割手。"]
[14,"单通工作柜","1800*800*800","台",3,"优质不锈钢制造，主体1.5mm不锈钢板材，下滑轮冲压轨道门，中间层板1.2mm，配备可调式不锈钢子弹脚，直径50mm，防割手。"]
[15,"保鲜工作台","1800*800*800","台",2,"不锈钢磨砂面板、环保制冷剂、防霉抑菌技术、自动回归门、可调子弹脚。冷藏0ºC~+10ºC，制冷剂134A;全铜管,柜体内,外均采用不锈钢板制作，自动回位门。"]
[16,"双层工作台","1800*800*800","台",1,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[17,"菜墩菜刀消毒柜","1200*700*1500","台",1,"整体不锈钢箱体，双门采用钢化玻璃，紫外线消毒，电压：220V，功率：1.2KW。"]
[18,"四门冰箱","1220*700*1800","台",2,"全不锈钢板材，品牌压缩机，双机双温，箱内高强度加厚铜管，门体自动复位，整体发泡层，220V/50HZ。"]
[null,"    面点加工"]
[1,"压面机","60#","台",1,"食品级不锈钢，铜包电机，可揉面压面，多种面条刀可随意切换"]
[2,"和面机","50kg","台",1,"食品级不锈钢，铜包电机，电压380V,功率1.5kw，"]
[3,"拌陷机",null,"台",1,"采用食品级不锈钢制作。平行浆叶式双轴结构设计，料斗内无死角设计。"]
[4,"包子机",null,"台",1,"304食品级不锈钢机身，多功能使用，自动调节。双绞轮设计，独立成型。"]
[5,"烤箱","三层六盘","台",1,"不锈钢材质，独立控温，380V,20KW，风机延时断电功能，MCCB过载保护，温度分布均匀，360度旋转烘烤功能"]
[6,"电饼铛","45#","台",2,"自动恒温，电压：220V/380V，功率：5KW，产量≥30KG/小时，全201不锈钢外形设计。"]
[7,"炸锅","双缸","台",1,"双缸双筛，优质不锈钢，防干烧，电热自控，380v，功率12kw。"]
[8,"双门蒸车","1000*900","台",2,"24盘，全不锈钢，蒸盘为食品级304不锈钢。电压：380V，功率：24KW，整体全发泡层，保温节能时长≥5h，自动进水停水系统。"]
[9,"木面案工作台","1800*800*800","台",3,"采用优质不锈钢制造，主体用1.5mm不锈钢板材，50mm柳木案板，不锈钢5cm圆管腿，壁厚1.2mm，可调节重力防滑子弹脚，防割处理。"]
[10,"单星水池","600*800*800","台",1,"采用不锈钢板1.35mm，星盆为一次冲压成型，配备不锈钢过滤、防臭下水漏；支撑腿厚度1.2mm,直径为50mm圆钢,可调节高度不锈钢子弹脚。"]
[11,"四门冰箱","1220*700*1800","台",1,"全不锈钢板材，品牌压缩机，双机双温，箱内高强度加厚铜管，门体自动复位，整体发泡层，220V/50HZ。"]
[12,"醒发箱","单门","台",1,"采用不锈钢层架，可调节，可拆卸。带风机热循环，电脑控制。"]
[13,"饼盘车","12层","台",1," 采用优质不锈钢板，板材厚度1.5mm，不锈钢钢管支撑腿，厚度1.2mm，直径50mm，表面抛光处理，可调节不锈钢子弹脚。"]
[null,"     凉菜间"]
[1,"预进间水池","650*760*800","台",1,"采用不锈钢板1.35mm，星盆为一次冲压成型，配备不锈钢过滤、防臭下水漏；支撑腿厚度1.2mm,直径为50mm圆钢,可调节高度不锈钢子弹脚。"]
[2,"双星水池","1200*760*800","台",1,"采用不锈钢板1.35mm，星盆为一次冲压成型，配备不锈钢过滤、防臭下水漏；支撑腿厚度1.2mm,直径为50mm圆钢,可调节高度不锈钢子弹脚。"]
[3,"双层工作台","2000*800*800","台",2,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[4,"保鲜工作台","1800*800*800","台",1,"不锈钢磨砂面板、环保制冷剂、防霉抑菌技术、自动回归门、可调子弹脚。冷藏0ºC~+10ºC，制冷剂134A;全铜管,柜体内,外均采用不锈钢板制作，自动回位门。"]
[5,"备餐柜","1800*700*800","台",1,"采用优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[6,"送餐车","100*730","台",2," 采用优质不锈钢面板，厚1.5mm，40不锈钢管支撑管，配可活动脚，带刹导轮。"]
[null,"    粗加工"]
[1,"浸泡池","1000*800*800","台",6,"采用不锈钢板1.35mm，星盆为一次冲压成型，配备不锈钢过滤、防臭下水漏；支撑腿厚度1.2mm,直径为50mm圆钢,可调节高度不锈钢子弹脚。"]
[2,"热水器","80L","台",1,"名牌，功率3KW。"]
[3,"四层货架","1400*800*1550","台",1,"高强度不锈钢板，厚1.2mm，支撑腿选用高强度不锈钢无缝钢管，单层承重60-100Kg；可调节高度的不锈钢子弹脚。"]
[4,"绞肉机","立式","台",1,"不锈钢加厚材质，铜包电机，进口齿轮，多功能绞切。"]
[5,"多功能切菜机",null,"台",1,"数控调节，电压，220V.功率3.15KW,净重160KG，产品功能，可切丝、切片、切丁，切段。"]
[6,"去皮机",null,"台",1,"滚筒毛刷式，电压，220V.功率1.5KW,净重100KG，直径750，桶深30cm，产量450KG/h"]
[7,"双层工作台","1800*800*800","台",4,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[null,"     洗碗间"]
[1,"单眼收餐台","800*700*800","台",1,"优质不锈钢，台面1.5mm,层架1.2mm，防割手。"]
[2,"浸泡池","1000*700*800","台",2,"采用优质不锈钢板1.35mm，星盆为一次冲压成型，配备不锈钢过滤、防臭下水漏；支撑腿厚度1.2mm,直径为50mm,可调节高度不锈钢子弹脚。"]
[3,"污碟台","1100*700*800","台",1,"采用优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[4,"洗碗机带烘干","长龙式","台",1,"全自动机械控制，双道清洗槽，380V/58KW，带烘干"]
[5,"洁碟台","1100*700*800","台",1,"采用优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[6,"热水器","80L","台",1,"名牌，功率3KW"]
[7,"高温消毒柜","双门","台",1,"板材选用优质304不锈钢板，板材厚度1.2mm的不锈钢板，高温热风循环定时消毒系统。"]
[8,"四层碗柜","1200*500*1800","台",1,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[9,"米面架","1200*600*300","台",1,"高强度不锈钢板，层板厚1.5mm，面板能承受≥1500KG/M2平均载荷。不锈钢可调节重力子弹脚，防割手。"]
[10,"四层货架","1200*500*1800","台",2,"高强度不锈钢板，厚1.2mm，支撑腿选用高强度不锈钢无缝钢管，单层承重60-100Kg；可调节高度的不锈钢子弹脚。"]
[null,"     明档"]
[1,"双层工作台","1800*800*800","台",2,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[2,"双层工作台","1200*800*800","台",1,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[3,"五格保温售饭台","1800*800*800","台",3,"全不锈钢机身、304不锈钢汤盆，面板1.35mm厚，其它为1.2mm，冲压免边处理防止割手工艺，全自动控温，电力保护系统，可调子弹防滑脚。"]
[4,"麻辣汤炉","6眼","台",1,"面板采用1.35mm厚优质不锈钢板，内壳采用1.2mm不锈钢磨砂板，名牌电机配备安全保护系统，符合国家食品卫生标准。"]
[5,"木面案工作台","1700*800*800","台",1,"采用优质不锈钢制造，主体用1.5mm不锈钢板材，50mm柳木案板，不锈钢5cm圆管腿，壁厚1.2mm，可调节重力防滑子弹脚，防割处理。"]
[6,"煮面炉","900*800*800","台",2,"食品级304不锈钢，厚度1.2m，台面下衬板1.2mm，防割手工艺，微电脑高感应探头，电源220V，可调子弹防滑脚。"]
[null,"     库房"]
[1,"米面架","800*400*600","台",9,"高强度不锈钢板，层板厚1.5mm，面板能承受≥1500KG/M2平均载荷。不锈钢可调节重力子弹脚，防割手。"]
[2,"四层货架","1200*500*1550","台",8,"高强度不锈钢板，厚1.2mm，支撑腿选用高强度不锈钢无缝钢管，单层承重60-100Kg；可调节高度的不锈钢子弹脚。"]
[3,"冷库","3700*7500*2500","m3",69,"防腐蚀，防阻燃，5匹双控系统，优质冷风机及压缩机组。"]
[4,"四层货架","1200*500*1550","台",10,"高强度不锈钢板，厚1.2mm，支撑腿选用高强度不锈钢无缝钢管，单层承重60-100Kg；可调节高度的不锈钢子弹脚。"]
[null,"      餐厅"]
[1,"单眼收餐车","750*800*800","台",1,"优质不锈钢，台面1.5mm,层架1.2mm，防割手。"]
[2,"双层工作台","1800*800*800","台",1,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[3,"净水开水器","60L","台",1,"柜式按压龙头开水器，380V/12KW，三级过滤器，RO膜反渗透。"]
[4,"洗手池带柜","2500*600*800","台",1,"采用优质不锈钢板1.35mm，星盆为一次冲压成型，配备不锈钢过滤、防臭下水漏；支撑腿厚度1.2mm,直径为50mm,可调节高度不锈钢子弹脚。"]
[5,"六门更衣柜","900*400*1850","组",4,"铁皮1.0mm材质"]
[6,"餐盘消毒柜","单门","台",1,"板材选用优质304不锈钢板，板材厚度1.2mm的不锈钢板，紫外线灭菌，循环定时消毒系统。"]
[7,"长方桌椅","2400*1200","套",1,"台面选用石纹色，高密度板桌面，无拼接，抗压强，质感光滑。桌椅腿采用加厚加粗管材制作。"]
[8,"自助餐台","4600*800*800","套",1,"大理石台面采用钢挂结构，内有方管支架，配有LED灯光，220V电源插头，防漏电设计。整体餐台采用螺丝固定，可拆解方便移动。"]
[9,"布菲炉","长方形","台",4,"优质不锈钢板制作，食品级304不锈钢台盆，数控电加热。"]
[10,"布菲炉汤炉","圆形","台",2,"优质不锈钢板制作，食品级304不锈钢台盆，数控电加热。"]
["二层"]
[null,"名称","规格","单位","数量","参数"]
["     洗碗间"]
[1,"单眼收餐台","1000*800*800","台",1,"优质不锈钢，台面1.5mm,层架1.2mm，防割手。"]
[2,"浸泡池","1000*800*800","台",1,"采用不锈钢板1.35mm，星盆为一次冲压成型，配备不锈钢过滤、防臭下水漏；支撑腿厚度1.2mm,直径为50mm圆钢,可调节高度不锈钢子弹脚。"]
[3,"热水器","80L","台",1,"名牌,功率3KW"]
[4,"污碟台","1200*800*800","台",1,"采用优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[5,"洗碗机带烘干","长龙式","台",1,"全自动机械控制，双道清洗槽，380V/58KW，带烘干"]
[6,"洁碟台","1200*800*800","台",1,"面板采用1.5mm厚优质不锈钢板，其它为1.2mm不锈钢，不锈钢无缝钢管支撑腿，厚度为1.2mm，直径为50mm，表面抛光，可调节高度不锈钢子弹脚。"]
[7,"双层工作台","960*500*800","台",1,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[8,"四层货架","1200*500*1550","台",2,"高强度不锈钢板，厚1.2mm，支撑腿选用高强度不锈钢无缝钢管，单层承重60-100Kg；可调节高度的不锈钢子弹脚。"]
[9,"四层碗柜","1200*500*1800","台",2,"采用优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[10,"高温消毒柜","1200*600*1800","台",3,"板材选用优质304不锈钢板，板材厚度1.2mm的不锈钢板，紫外线灭菌，高温热风循环定时消毒系统。"]
[11,"洗手池带柜","2000*600*800","台",1,"采用优质不锈钢板1.35mm，星盆为一次冲压成型，配备不锈钢过滤、防臭下水漏；支撑腿厚度1.2mm,直径为50mm,可调节高度不锈钢子弹脚。"]
[12,"双眼收餐台","1200*800*800","台",1,"采用优质不锈钢，台面1.5mm,层架1.2mm，防割手。"]
[13,"双层工作台","1200*800*800","台",2,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[14,"四人桌椅","1200*600","套",63,"高防实木制作，椅子可活动。"]
[15,"六人桌椅","1500*600*800","套",4,"高防实木制作，椅子可活动。"]
[16,"自助餐台","9000*1600","套",1,"大理石台面采用钢挂结构，内有方管支架，配有LED灯光，220V电源插头，防漏电设计。整体餐台采用螺丝固定，可拆解方便移动。"]
[17,"布菲炉","长方形","台",14,"优质不锈钢板制作，食品级304不锈钢台盆，数控电加热。"]
[18,"布菲炉汤炉","圆形","台",6,"优质不锈钢板制作，食品级304不锈钢台盆，数控电加热。"]
[19,"工作台","1800*600*800","台",1,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
["     明档"]
[1,"木面案工作台","1500*750*800","台",1,"采用优质不锈钢制造，主体用1.5mm不锈钢板材，50mm柳木案板，不锈钢5cm圆管腿，壁厚1.2mm，可调节重力防滑子弹脚，防割处理。"]
[2,"四格保温售饭台","1500*700*800","台",1,"全不锈钢机身、304不锈钢汤盆，面板1.35mm厚，其它为1.2mm，冲压免边处理防止割手工艺，全自动控温，电力保护系统，可调子弹防滑脚。"]
[3,"煮面炉","600#","台",2,"采用优质不锈钢制作，内圆外方。干烧加热管设计，内外均匀，复底桶设计。"]
[4,"保鲜工作台","1800*800*800","台",1,"不锈钢磨砂面板、环保制冷剂、防霉抑菌技术、自动回归门、可调子弹脚。冷藏0ºC~+10ºC，制冷剂134A;全铜管,柜体内,外均采用不锈钢板制作，自动回位门。"]
[5,"单通工作台","1800*800*800","台",2,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[6,"双星水池","1200*700*800","台",1,"采用不锈钢板1.35mm，星盆为一次冲压成型，配备不锈钢过滤、防臭下水漏；支撑腿厚度1.2mm,直径为50mm圆钢,可调节高度不锈钢子弹脚。"]
[7,"双层工作台","1500*700*800","台",1,"优质不锈钢制造，台面1.5mm不锈钢板材，层板1.2mm，脚为直径50mm*壁厚1.2mm不锈钢无缝钢管，表面抛光处理，不锈钢可调节重力子弹脚，防割手。"]
[8,"餐车","三层","台",1,"采用优质不锈钢，厚1.5mm，40不锈钢管支撑管，配可活动脚，带刹导轮。"]
[9,"宴会保温车","单门","台",2,"优质钢板厚度板材厚度1.2m，台面下衬板为1.2mm，全自动控温系统及电力保护系统，防割手工艺，可调子弹防滑脚。\n"]
["排风"]
[1,"名称","规格","单位","数量","参数"]
[2,"玻璃烟罩","5m*1m*500","m²",5,"优质不锈钢制造，主体用1.2mm不锈钢板材。可调式出风口，接油盒，板式防火挡板，封闭式防潮防爆灯。"]
[3,"排烟罩","11.6m*1300*500","m²",15,"优质不锈钢制造，主体用1.2mm不锈钢板材，板式防火挡板，封闭式防潮防爆灯。"]
[4,"排烟罩","8900*1200*500","m²",10.68,"优质不锈钢制造，主体用1.2mm不锈钢板材，板式防火挡板，封闭式防潮防爆灯。"]
[5,"排烟罩","2500*1200*500","m²",3,"优质不锈钢制造，主体用1.2mm不锈钢板材，板式防火挡板，封闭式防潮防爆灯。"]
[6,"烟筒","1200#","m²",85,"优质镀锌板1.2mm"]
[7,"三通","1200#","个",1,"优质镀锌板1.2mm"]
[8,"烟筒","600#","m²",118,"优质镀锌板1.2mm"]
[9,"弯头","600#","个",2,"优质镀锌板1.2mm"]
[10,"三通","600#","个",3,"优质镀锌板1.2mm"]
[11,"堵头","600#","个",4,"优质镀锌板1.2mm"]
[12,"弯头","1200#","个",3,"优质镀锌板1.2mm"]
[13,"外法兰","1200#","对",26,"4#角钢，防锈处理。"]
[14,"外法兰","600#","对",14,"4#角钢，防锈处理。"]
[15,"烟筒支架","1100#","套",4,"4#角钢，防锈处理。"]
[16,"风柜","600#","台",1,"全铜国标电动机，双层静音，高效高压。"]
[17,"净化器","40A","台",1,"可自动调节电场强度，保持净化效率，达95效果。"]
[18,"变频控制箱","18.5KW ","套",1,"漏电缺项保护，可调电机转速。"]
[19,"风柜变径","1350#","个",4,"优质镀锌板1.2mm"]
[20,"减震装置","360KG","套",4,"橡胶减震"]
[21,"风柜","315#","台",1,"全铜国标电动机，双层静音，高效高压。"]
[22,"净化器","12A","台",1,"可自动调节电场强度，保持净化效率，达95效果。"]
[23,"变频控制箱","4KW","套",1,"漏电缺项保护，可调电机转速。"]
[24,"吊杆",null,"对",26,"10#丝杆"]
[25,"烟筒","660#","m²",40,"优质镀锌板1.2mm"]
[26,"弯头","660#","个",2,"优质镀锌板1.2mm"]
[27,"外法兰","660#","对",10,"4#角钢，防锈处理。"]
["新风"]
[1,"名称","规格","单位","数量","参数"]
[2,"烟筒","800#","m²",35,"优质镀锌板1.2mm"]
[3,"三通","800#","个",2,"优质镀锌板1.2mm"]
[4,"弯头","800#","个",2,"优质镀锌板1.2mm"]
[5,"烟筒","600#","m²",20,"优质镀锌板1.2mm"]
[6,"变径","600#","个",4,"优质镀锌板1.2mm"]
[7,"外法兰","800#","对",20,"4#角钢，防锈处理"]
[8,"新风百叶","300*300","套",10,"不锈钢板材，板材厚1.0mm"]
[9,"空气过滤箱",null,"套",1,"优质不锈钢1.2mm，双层空气过滤网"]
[10,"吊杆",null,"对",12,"10#丝杆"]
[11,"静音风柜","450#","台",1,"全铜国标电动机，双层静音，高效高压。"]
[12,"风柜变径","1100#","个",2,"优质镀锌板1.2mm"]
[13,"吊装减震","320KG","套",1,"橡胶减震"]
[14,"出口百叶","800#","套",1,"优质不锈钢1.2mm，双层空气过滤网。"]
[15,"变频控制箱","5.5KW","套",1,"漏电缺项保护，可调电机转速。"]
[16,"外法兰","600#","对",6,"帆布软接"]
[17,"烟筒","500#","m²",15,"优质镀锌板1.2mm"]
["餐具"]
[1,"名称","规格","单位","数量","参数"]
[2,"自助餐盘","五格","个",1000,"密胺材质，高防瓷"]
[3,"大碗","8.5#","个",500,"密胺材质，高防瓷"]
[4,"中碗","7.5#","个",500,"密胺材质，高防瓷"]
[5,"小碗","5#","个",1000,"密胺材质，高防瓷"]
[6,"筷子",null,"双",1200,"密胺材质"]